# Story 3.1: Stale State Detection & Dimmed Display

Status: done

## Story

As a user whose RTL-SDR has temporarily lost signal,
I want the display to retain the last known aircraft positions shown as outlines when dump1090 stops delivering fresh data,
So that I know the display is stale without a crash or blank screen.

## Acceptance Criteria

AC1: **Given** the radar loop is running with a previous successful fetch **When** `HttpFetcher.fetch()` raises `requests.Timeout` **Then** the exception propagates to the loop boundary, which catches it and marks all retained aircraft as `is_stale=True`

AC2: **Given** the dump1090 response returns an empty aircraft list when the previous cycle had aircraft **When** the fetcher processes the response **Then** the previous aircraft list is retained with `is_stale=True` on each entry (not replaced with empty)

AC3: **Given** aircraft with `is_stale=True` are passed to the renderer **When** `renderer.render()` is called **Then** each stale aircraft is drawn as outline only using `COLOUR_STALE_OUTLINE` **And** heading arrow, label, and trail are still rendered at last known positions

AC4: **Given** a stale render cycle **When** the render loop timing is measured **Then** the loop does not crash (stale path is not a crash path)

## Tasks / Subtasks

- [x] Task 1: Update `_run_one_cycle()` and `main()` in `src/planemapper/main.py` (AC: #1, #2, #4)
  - [x] 1.1 Add `last_aircraft: list[Aircraft]` parameter to `_run_one_cycle`; change return type to `list[Aircraft]`
  - [x] 1.2 Wrap `fetcher.fetch()` in `try/except requests.Timeout`
  - [x] 1.3 Implement stale logic: use `last_aircraft` with `is_stale=True` when timeout or empty+had-previous
  - [x] 1.4 Update `main()` to initialise `last: list[Aircraft] = []` and track return value of `_run_one_cycle`
  - [x] 1.5 Add `import dataclasses` and `import requests` to `main.py`

- [x] Task 2: Update `draw_aircraft()` in `src/planemapper/renderer/aircraft.py` (AC: #3)
  - [x] 2.1 Import `COLOUR_STALE_OUTLINE` from `planemapper.constants`
  - [x] 2.2 Check `aircraft.is_stale` before calling `_draw_arrow`: if stale, use `COLOUR_STALE_OUTLINE` with forced outline mode

- [x] Task 3: Write tests in `tests/test_stale.py` (AC: #1, #2, #3, #4)
  - [x] 3.1 Test AC1: mock `fetcher.fetch()` to raise `requests.Timeout`; call `_run_one_cycle` with `last_aircraft=[some_aircraft]`; assert returned list has `is_stale=True`
  - [x] 3.2 Test AC2: mock `fetcher.fetch()` to return `[]`; call with non-empty `last_aircraft`; assert returned list has `is_stale=True`
  - [x] 3.3 Test AC3: render stale aircraft; assert pixel at aircraft position is not the altitude colour (stale colour is `COLOUR_STALE_OUTLINE` = black)
  - [x] 3.4 Test AC4: full stale cycle with renderer completes without exception

- [x] Task 4: Run quality gates
  - [x] 4.1 `python -m pytest tests/` — all tests pass
  - [x] 4.2 `python -m ruff check .` — zero violations
  - [x] 4.3 `python -m ruff format --check .` — no formatting issues

## Implementation Notes

### Key insight: `is_stale` already exists

The `is_stale` field already exists on the `Aircraft` dataclass (defaults to `False`). No model changes are needed. The `is_mlat` field already drives outline rendering in `_draw_arrow` — stale aircraft reuse the same outline path but with a different colour.

### Stale vs MLAT rendering distinction

| Condition | Fill | Outline colour | Meaning |
|---|---|---|---|
| Normal | altitude colour | — | Direct ADS-B, current data |
| MLAT (`is_mlat=True`) | None | altitude colour | Uncertain position, current data |
| Stale (`is_stale=True`) | None | `COLOUR_STALE_OUTLINE` (black) | Last known position, data age unknown |

Stale takes priority over MLAT in the rendering check: if `aircraft.is_stale` is true, always render outline in `COLOUR_STALE_OUTLINE` regardless of `is_mlat`.

### `_run_one_cycle` signature change

```python
def _run_one_cycle(
    renderer: Renderer,
    fetcher: HttpFetcher,
    display: DisplayInterface,
    last_aircraft: list[Aircraft],
) -> list[Aircraft]:
```

Returns the aircraft list used for this cycle (caller passes it back as `last_aircraft` next cycle).

### Stale detection logic in `_run_one_cycle`

```python
try:
    fresh = fetcher.fetch()
except requests.Timeout:
    log.warning("fetch timeout — using stale data")
    fresh = []
    stale_needed = True
else:
    stale_needed = (len(fresh) == 0 and len(last_aircraft) > 0)

if stale_needed:
    aircraft_list = [dataclasses.replace(a, is_stale=True) for a in last_aircraft]
else:
    aircraft_list = fresh
```

`dataclasses.replace()` creates a new `Aircraft` instance with only `is_stale` changed — the original `last_aircraft` entries are not mutated.

### `main()` loop update

```python
last: list[Aircraft] = []
while True:
    last = _run_one_cycle(renderer, fetcher, display, last)
    time.sleep(REFRESH_INTERVAL_S)
```

Initialise `last` as empty list before the loop. On first cycle, `last_aircraft=[]` means a timeout or empty result produces an empty stale list (no aircraft to retain), which renders a clean empty map — correct behaviour.

### `draw_aircraft()` stale check

In `src/planemapper/renderer/aircraft.py`, inside `draw_aircraft()`, before calling `_draw_arrow`:

```python
if aircraft.is_stale:
    _draw_arrow(draw, cx, cy, aircraft.heading, COLOUR_STALE_OUTLINE, is_mlat=True)
else:
    _draw_arrow(draw, cx, cy, aircraft.heading, colour, aircraft.is_mlat)
```

The `is_mlat=True` argument reuses the existing outline-only code path in `_draw_arrow`. The label and trail draw unconditionally at the last known positions — stale state does not suppress them.

### Required imports in `main.py`

- `import dataclasses` — for `dataclasses.replace()`
- `import requests` — to name `requests.Timeout` in the `except` clause

Both should be added to the top-level imports alongside the existing ones.

### Files changed

| File | Change |
|---|---|
| `src/planemapper/main.py` | Add params/return to `_run_one_cycle`; stale detection logic; update `main()` loop; add imports |
| `src/planemapper/renderer/aircraft.py` | Import `COLOUR_STALE_OUTLINE`; stale check before `_draw_arrow` |
| `tests/test_stale.py` | New test module covering all four ACs |
